**OCFS SPORTSMAN RULES REVISIONS April 9, 2022**

Rules revision to Section S50B , Carburetor .

#2 - Up to a 1” thick unaltered single hole carburetor spacer is allowed. No tapering or other machining is permitted. Two conventional gaskets will be allowed to reach a maximum overall total thickness of 1 1/8”. Shape of spacer opening must be configured in a Squircle shape…ie straight sides with radiused corners. Spacer material is optional.

Rules revision to S50H , Claimer.

#2 - Cost to claim a Sportsman engine will now be $6,000.